**GEDA 1200 Z/ZP Hoist Type C.**

Available for 15m lifting height, 5x landing level, Platform C and roof.

|  |  |  |
| --- | --- | --- |
| **Description** | **No. Units** | **Total Weight** |
|  |  |  |
| GEDA 1200 ZZP Platform C Roof (63172) | 1 | 0 |
| GEDA Extension cord 20m (2513) | 1 | 4.4 |
| GEDA Landing level safety gate comfort (1212) | 5 | 330 |
| GEDA Electric set (1214) | 1 | 3.2 |
| GEDA Central spindle (E020310) | 1 | 6.8 |
| GEDA 1200ZZP Steel mast 1.5m (E020300) | 10 | 820 |
| GEDA Trailing cable guide (E020265) | 4 | 11.6 |
| GEDA 1200 ZZP with stage "C" (E120254) | 1 | 0 |
| GEDA Cable bin 50m (E120261) | 1 | 0 |
| Set of mast ties P12/ERA (51610) | 3 | 0 |
| GEDA 1200ZZP Assembly plank | 1 | 0 |
| GEDA 1200ZZP Craning device | 1 | 0 |

**Technical Data**

|  |  |
| --- | --- |
| **Cargo** | Personnel and material |
| **Mast system** | GEDA VARIO-MAST |
| **Load Capacity (material)** | 1000kg |
| **Load capacity (persons)** | 7 persons |
| **Lifting Height** | 150m (max) |
| **Lifting Speed** | 12m/min / 24m/min |
| **Power supply** | 2 x 3 kW / 6.1kW / 400 V / 50 Hz / 32A |
| **Platform dimensions** | 1.4m x 3.2m x 1.1m/1.8m |

