**GEDA 1500Z/ZP Hoist Platform BS**

Available for 30m lifting height, 10 x landing levels, Platform BS and roof.

|  |  |  |
| --- | --- | --- |
| **Description** | **No. Units** | **Total Weight** |
|  |  |  |
| GEDA 1500ZZP Base roof (1010444) | 1 | 0 |
| GEDA 1500ZZP Roof extension 1.4m x 0.6m (1010557) | 1 | 0 |
| GEDA 1500ZZP Diagnostic system (45573) | 1 | 2.5 |
| GEDA 500ZZP Steel mast 1.5m (1150) | 40 | 1760 |
| GEDA Trailing cable guide (1165) | 5 | 13.5 |
| GEDA Extension cord 20m (2513) | 1 | 4.4 |
| GEDA 1500ZZP Base unit (2606) | 1 | 970 |
| GEDA Limit switch for 300/500/1500 ZZP landing level (2628) | 9 | 29.7 |
| GEDA cable bin with trailing cable 50m (1231) | 1 | 90 |
| GEDA 1500ZZP set of mast ties x2 for wall fixing | 4 | 240 |
| GEDA landing level safety gate comfort (1212) | 10 | 660 |
| GEDA electric set (1214) | 10 | 32 |
| GEDA Assembly plank (2626) | 2 | 80 |
| GEDA 1500ZZP platform BS (2642) | 1 | 610 |

**Technical Data**

|  |  |
| --- | --- |
| **Cargo** | Personnel and material |
| **Mast system** | GEDA UNI-MAST |
| **Load Capacity (material)** | 2000kg |
| **Load capacity (persons)** | 7 persons |
| **Lifting Height** | 100m (max) |
| **Lifting Speed** | 12m/min / 24m/min |
| **Power supply** | 2 x 3 kW / 6.1kW / 400 V / 50 Hz / 32A |
| **Platform dimensions** | 1.45m x 3.3m x 1.1m/1.8m |

